| **DESCRIPTION** | **WEIGHT/UNIT(KG)** |
| --- | --- |
| Base Jacks | 4.4 |
| U Jacks | 4.4 |
| 3m Standards | 14.8 |
| 2.5m Standards | 12.3 |
| 2m Standards | 10.2 |
| 1.5m Standards | 7.6 |
| 1m Standards | 5 |
| 0.5m Standards | 2.5 |
| 2.5m Ledgers | 8 |
| 2m Ledgers | 6.5 |
| 1.5m Ledgers | 5.5 |
| 1.3m Ledgers | 4.4 |
| 1.2m Ledgers | 4.4 |
| 900mm Ledgers | 3.2 |
| 600mm Ledgers | 2.2 |
| 2.5m Steel Boards | 18 |
| 2.0m Steel Boards | 15.93 |
| 1.3m Steel Boards | 9.15 |
| 900mm Steel Boards | 7.55 |
| No. Acro Props | 22 |
| 2.5m Toe Boards | 14.3 |
| 2.0m Toe Boards | 11.6 |
| 1.3m Toe Boards | 7.8 |
| Toe Board Clips | 0.5 |
| Band and Plate Sets | 1.8 |
| Swivel Couplers | 0.2 |
| 6m Bracing Tubes | 22 |
| 3m Bracing Tubes | 11 |
| Castor Wheels | 5 |
| 2m Ladders | 27 |
| 2m Staircase and Handrail | 65 |
| Trapdoor | 16.01 |
| Ledger Beams | 48 |